**Channel Cross Section Datasheet**

|  |  |
| --- | --- |
| **Date:** | **Observer(s):** |
| **Site (i.e. NNWR):** | **Location (i.e. U3N):** |
|  | |
| **Endpoint Marker 1:** | **Endpoint Marker 2:** |
| **Bank Location (i.e. N, S, E, W)** | **Bank Location (i.e. N, S, E, W)** |
| **UTM Northing:** | **UTM Northing:** |
| **UTM Easting:** | **UTM Easting:** |
| **Distance from level line to top of endpoint marker (m):** | **Distance from level line to top of endpoint marker (m):** |
|  | |
| **Starting Bank (i.e. N, S, E, W):** | **Total Channel Width (m):** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Distance along channel (0.5 m increments)** | **Height to level line (m)** | **Notes** | **Distance along channel (0.5 m increments)** | **Height to level line (m)** | **Notes** |
| **0** |  |  | **13.0** |  |  |
| **0.5** |  |  | **13.5** |  |  |
| **1.0** |  |  | **14.0** |  |  |
| **1.5** |  |  | **14.5** |  |  |
| **2.0** |  |  | **15.0** |  |  |
| **2.5** |  |  | **15.5** |  |  |
| **3.0** |  |  | **16.0** |  |  |
| **3.5** |  |  | **16.5** |  |  |
| **4.0** |  |  | **17.0** |  |  |
| **4.5** |  |  | **17.5** |  |  |
| **5.0** |  |  | **18.0** |  |  |
| **5.5** |  |  | **18.5** |  |  |
| **6.0** |  |  | **19.0** |  |  |
| **6.5** |  |  | **19.5** |  |  |
| **7.0** |  |  | **20.0** |  |  |
| **7.5** |  |  | **20.5** |  |  |
| **8.0** |  |  | **21.0** |  |  |
| **8.5** |  |  | **21.5** |  |  |
| **9.0** |  |  | **22.0** |  |  |
| **9.5** |  |  | **22.5** |  |  |
| **10.0** |  |  | **23.0** |  |  |
| **10.5** |  |  | **23.5** |  |  |
| **11.0** |  |  | **24.0** |  |  |
| **11.5** |  |  | **24.5** |  |  |
| **12.0** |  |  | **25.0** |  |  |
| **12.5** |  |  | **25.5** |  |  |